|  |
| --- |
| **PLANNED DITCHING – FORWARD EXITS** |
| **ABP BRIEFING CARD****BRIEF 4 ABP’s: 2 FOR LEFT EXIT, 2 FOR RIGHT EXIT** |
| **F/A ACTION** | **ABP BRIEFING** |
| **Brief ABP #1 & #2** | After plane comes to a stop in the water, we will open the doors to evacuate. If we cannot open the doors, you will be responsible.Come to this door. Remove me/us from the seat and place me/us in seat(s) in the first row. Look through the window. If there is danger outside, do not open the door. Block the exit and direct people to the opposite door. If it looks safe to open the door, hold the forward handle with one hand and use your other hand to lift the door handle up in the direction of the arrow. The door should open automatically. If it does not, push the door fully open. The slide/raft should immediately inflate automatically. If it does not inflate, pull on the red inflation handle in the doorsill to inflate. The one that opens the door must stand here, holding this handle. Repeatedly shout: “**OPEN SEATBELTS! LEAVE EVERYTHING! COME THIS WAY! GET OUT! INFLATE VEST! CRAWL TO THE END! SIT WITH YOUR BACK AGAINST THE TUBES! GO!”**When you are ready to exit the plane and get into the raft, grab me/us and put me/us in the slide/raft, then leave and pull on the quick release handle.**ABP #2:** After the slide/raft inflates, crawl to the end of the slide raft and make people sit with their backs against the tubes alternating sides to balance the raft. |
| Form # REV: 000 01/01/2021 |

|  |
| --- |
| **PLANNED DITCHING – OVERWING EXITS** |
| **ABP BRIEFING CARD****3 ABPs PER LIFE RAFT** |
| **F/A ACTION** | **ABP BRIEFING** |
| **Brief ABP #1** | After plane stops, if evacuation is necessary, I/we will come to the exit and take charge. If I/we cannot take charge, you take charge. |
| **Brief ABP #2 & #3***Show ABP’s location of rafts and equipment* | After plane stops, open this/these overhead compartment/s for the rafts. The raft inflation line is under this red pouch – this inflates the raft. Don’t pull it hard inside the plane.The raft is heavy – 2 people must lower it. Remove the life line from this compartment and give it to ABP #1. |
| **Brief ABP #1***Prepare to exit plane* | Once the life raft/s are down, look out this window. If there are sharp objects or the water level is too high, do not open the exit. Stay here. Tell ABPs 2 & 3 to bring the life raft to the opposite exit or another exit and tell the passengers to follow them.If it appears safe outside, open the exit. Take a Life Line, attach one hook to the ring in window frame and step outside. Then, inflate your life vest and attach the other end of the Life Line to the yellow ring on the wing.Then, come back and stand outside of the wing exit. |
| **Brief ABP #2 & #3** | After the Life Line is attached by ABP #1, carefully remove the inflation line and attach it to a fastened passenger seatbelt. Lift raft and step down onto the wing. Inflate one chamber of your vest. Carry the raft to the front of wing. Throw the raft into the water. Pull hard and repeatedly on the inflation line until the life raft inflates. When raft inflates, you (ABP #2) stay on wing.You (ABP #3) get into the raft. Help people climb into the raft, sit them down, back against tubes. Distribute weight evenly! |
| **Brief ABP #1** | When raft inflates, help people out and shout**: Inflate vest! Hold rope! Step onto wing!** When the raft is full or the plane is empty, then you get into the raft and cut the line to separate from the plane. **Study this card.** |
| Form # REV: 000 01/01/2021 |

|  |
| --- |
| **PLANNED DITCHING – AFT EXITS** |
| **ABP BRIEFING CARD****BRIEF 4 ABP’s: 2 FOR LEFT EXIT, 2 FOR RIGHT EXIT** |
| **F/A ACTION** | **ABP BRIEFING** |
| **Brief ABP #1 & #2** | **ABP #1:** After the plane comes to a stop in the water, we will open the doors to evacuate. If we cannot open the doors, you will be responsible.Come to this door. Remove me/us from the seat and place me/us in seat(s) in the last row of seats. Look through the window. If the water level is high, do not open the door. Block the exit and direct people to the front of the plane. If it looks safe to open the door, hold the forward handle with one hand and use your other hand to lift the door handle up in the direction of the arrow. The door should open automatically. If it does not, push the door fully open. The slide/raft should immediately inflate automatically. If it does not inflate, pull on the red inflation handle in the doorsill to inflate. The one that opens the door must stand here, holding this handle. Repeatedly shout: “**OPEN SEATBELTS! LEAVE EVERYTHING! COME THIS WAY! GET OUT! INFLATE VEST! CRAWL TO THE END! SIT WITH YOUR BACK AGAINST THE TUBES! GO!”**When you are ready to exit the plane and get into the raft, grab me/us and put me/us in the slide/raft, then leave and pull on the quick release handle.**ABP #2:** After the slide/raft inflates, crawl to the end of the slide raft and make people sit with their backs against the tubes alternating sides to balance the raft.Study this card. |
| Form # REV: 000 01/01/2021 |